**STAMPE**

|  |  |  |  |
| --- | --- | --- | --- |
|  | **RPM** | **TIME** | **OIL** |
| **TAKEOFF** | **2150** | **60mins** | **30-40** |
| **CRUISE** | **2000** | **CONT** | **30-40** |
| **MAX** | **2400** | **5 mins** | **30-40** |
| **MAX O/S** | **2520** |  |  |

 **Vne - 148kts. MAUM - 825kg MAero - 770kg**

 **/176mph ZFW - 563kg**

|  |  |
| --- | --- |
| ***RUN-UP*****1700 rpm - 2 min 2000 rpm - 10 sec****MAGDROP 75 rpm****IDLE - 400rpm****Min Oil Pres 30 psi** | ***PRE TAKE OFF*****T - TRIM CENTRE****T - THROTTLE****M - MIX RICH****M - MAGS BOTH****F - FUEL ON/CONT****G - GUAGES****H - HATCH / HARN****C - CONTROLS****E - ENGINE RESP** |
| ***LANDING*****B - BRAKES****M - MIXTURE****F - FUEL****H - HARNESSES** | ***AEROS*****LOOP - 100****BARREL - 100****SLOW - 95****ROLL O' TOP - 120****STALL TURN - 100** |