**STAMPE**

|  |  |  |  |
| --- | --- | --- | --- |
|  | **RPM** | **TIME** | **OIL** |
| **TAKEOFF** | **2150** | **60mins** | **30-40** |
| **CRUISE** | **2000** | **CONT** | **30-40** |
| **MAX** | **2400** | **5 mins** | **30-40** |
| **MAX O/S** | **2520** |  |  |

**Vne - 148kts. MAUM - 825kg MAero - 770kg**

**/176mph ZFW - 563kg**

|  |  |
| --- | --- |
| ***RUN-UP***  **1700 rpm - 2 min 2000 rpm - 10 sec**  **MAGDROP 75 rpm**  **IDLE - 400rpm**  **Min Oil Pres 30 psi** | ***PRE TAKE OFF***  **T - TRIM CENTRE**  **T - THROTTLE**  **M - MIX RICH**  **M - MAGS BOTH**  **F - FUEL ON/CONT**  **G - GUAGES**  **H - HATCH / HARN**  **C - CONTROLS**  **E - ENGINE RESP** |
| ***LANDING***  **B - BRAKES**  **M - MIXTURE**  **F - FUEL**  **H - HARNESSES** | ***AEROS***  **LOOP - 100**  **BARREL - 100**  **SLOW - 95**  **ROLL O' TOP - 120**  **STALL TURN - 100** |